Escali Alimento
Calibration Procedures

1. Before turning on the scale, hold down the **Tare**, **Backlight**, and **Kg/Lb** buttons at the same time
2. While holding down the three buttons, press the **On/Off** button
3. The numbers **55555** will show on the screen; release the three buttons you are holding down, now press the **Back Light** button
4. The screen will now display random numbers; you will now press the **Tare** button
5. The message **2Ero** will display for one second, and then displays **6000g**
6. Gently place 6000g on the platform, and press the **Tare** button
7. The message **CAL** will display on the screen for a second, and then will display **PASS** if calibration is successful. (**EEEEE** will display if calibration was incorrectly done.)

Calibration complete